**KENT KVV225/1.5”BSP - Commercial Gully (Vinyl Floor)**

This is a modified version of our KVV225/110 Floor Gully to suit a 1 ½“ BSP or 2” BSP bottom outlet. It is supplied as standard with a lockdown plain top grating.

**Features**:

* Grade 304 (1.4301) or 316 (1.4401) Stainless Steel to BS EN 10088
* Satin finish as standard
* Lock down as standard