NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVV225110TP)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVV225110TP)

Product Specification:

KVV225/110TP

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Commercial Gully (Vinyl Floor)

• Type: KHV225/1.5"BSP /KHV225/1.5"BSP (PF) /KHV225/50 /KHV225/50 (PF) /KVV225/1.5"BSP 75 /KVV225/1.5"BSP(T) /KVV225/110 /KVV225/110 (PF) /KVV225/110TP /KVV225/110TP (PF) /KVV225/2"BSP /KVV225/2"BSP(T) /KVV225/50 /KVV225/50(T)

• Material: Grade 1.4301 (304) stainless steel /Grade 1.4401 (316) stainless steel

• Finish: Satin

• Outlet: 110mm

• Strainer: Not required /Required

Suggested Specification:

KVV225/110TP

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Commercial Gully (Vinyl Floor)

• Type: KVV225/110

• Material: Grade 1.4301 (304) stainless steel

• Finish: Satin

• Outlet: 110mm

• Strainer: Not required