NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/320 Covers, gratings and frames for access chambers

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[P30 Trenches, pipeways and pits for buried engineering services](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentTripleSealWaterTight)

* [301 ACCESS COVERS/ MANHOLE TOPS AND FRAMES](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Access-CoversKentTripleSealWaterTight)

Product Specification:

Kent Triple Seal Water Tight

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Triple Seal Water Tight Manhole

• Type: KMHT(W)-300/300 /KMHT(W)-450/450 /KMHT(W)-600/600 /KMHT(W)-750/750 /KMHT(W)-900/900

• Size: Bespoke /Manufacturer's standard

• Loading: FACTA AAA /FACTA B /FACTA C /FACTA D

• Material: 304L stainless steel /316L stainless steel

• Accessories: None /Enclosed fire-rated insulated panel

Suggested Specification:

Kent Triple Seal Water Tight

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Triple Seal Water Tight Manhole

• Type: KMHT(W)-600/600

• Size: 600mm x 600mm clear opening

• Loading: FACTA C

• Material: 316L stainless steel

• Accessories: Enclosed fire-rated insulated panel