NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesDoubleContainedGully)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesDoubleContainedGully)

Product Specification:

Double Contained Floor Drain Gully

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Double Contained Floor Drain Gully

• Type: KVCRDC265/4”/6” // KVCRDC6”/8”

• Loading class to BS EN 1253: L15 /R50 /M125 /N250 /P400

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Flange type: 4” 150lb R/F S/O ANSI flange /4” PN10 R/F S/O flange /Damp proof membrane flange /Holding flange /Puddle flange

• Grating: Kent Sealed Grating // Kent Slotted Grating // Kent Perforated Grating

• Filter basket: Not required /Required /Required, with chain /Required, with separate filter basket

• Accessories: None / Lockdown / Tundish / Staggered Ferrule Connections

Suggested Specification:

Double Contained Gully

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Double Contained Gully

• Type: KVCR265/4”/6”

• Loading class to BS EN 1253: M125

• Material: 1.4401 (316) stainless steel

• Flange type: None

• Grating: Kent Sealed Grating

• Filter basket: Not required

• Accessories: None