NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

Pop Up Outlet Channel Trench Drain

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +353 53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Pop Up Outlet Channel Trench Drain

• Type: KSBC450/KVCRP400/4” / KSBC450/KVCRP400/6”

• Loading class to BS EN 1253: L15 /R50 /M125 /N250 /P400

• Material: 1.4301 (304) stainless steel /1.4401 (316) stainless steel

• Flange type: 4” 150lb R/F S/O ANSI flange /4” PN10 R/F S/O flange /Damp proof membrane flange /Holding flange /Puddle flange

• Side inlets:

- Type: 1½” BSP nipple /1½” BSP socket /50 mm push fit /Above ground funnel

- Angle: 45° /90° /Bespoke

• Grating:

• Filter basket: Not required /Required /Required, with chain /Required, with separate filter basket

• Accessories:

Recommended Product Specification:

Pop Up Outlet Channel Trench Drain

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +353 53 914 3216

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Pop Up Outlet Channel Trench Drain

• Type: KSBC450/KVCRP400/4” / KSBC450/KVCRP400/6”

• Loading class to BS EN 1253: M125

• Material: 1.4401 (316) stainless steel

• Flange type: none

• Side inlets: none

• Grating: KLG Ladder Grating

• Filter basket: Not required

• Accessories: