NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor gullies

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVA205)

* [315 FLOOR DRAINS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-Internal-GulliesKVA205)

Product Specification:

KVA205

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: KVA205/110 /KVA205/110DS /KVA255/110 /KVA255/110DS /KVA355/160 /KVA355/160DS

• Material: Stainless steel, grade 304 (1.4301) /Stainless steel, grade 316 (1.4401)

• Grating:

• Accessories/ Other requirements: Not required /1 ½" BSP inlets /4” SCH10 Outlet /6” SCH10 Outlet /50 mm side inlets /Chained /Damp proof membrane /Filter basket /Foul air trap /Holding flange /Nipple (threaded outside) /Outlet flange /Puddle flange /Socket (threaded inside)

Suggested Specification:

KVA205

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: KVA205/110DS

• Material: Stainless steel, grade 304 (1.4301)

• Grating: KMG Kent Mesh Grating

• Accessories/ Other requirements: Filter basket